**Final Test Data Sample**

**RADIO SERVICES**

**including REFERENCE**

Version 08/10/2013

MARITIME RADIO STATIONS

|  |
| --- |
| **JUSSLAND** |

|  |  |  |  |
| --- | --- | --- | --- |
| **MARITIME TELEMEDICAL ASSISTANCE SERVICE (TMAS)** | | | |
| Usual name of centre | Jusslandcity Hospital, Jussland City | |  |
| Communications | Jussland MRCC : DSC A1 A2 A3 MMSI 005742029  Bonbonkrema MRSC : DSC A1 A2 A3 MMSI 005742030  Bonbonkrema (ZZZ) : DSC A1 A2 A3 MMSI 005742031 | | |
| Hospital Landlines : | | | |
|  +999(0)1 23456755-59 | |  +999(0)1 23456760 | |
| MRCC : | | | |
|  +999(0)1 23456789 | |  +999(0)1 23456788 | |
|  | | email: mrcc.jussland@jussland.gov.js | |
| Inmarsat C : +583 422123456  TELEX : +998 123456 | | WEBSITE : www.jussland.mrcc.js | |
| Associated MRCC or JRCC | MRCC JUSSLAND | | |
| Consultation Languages | Jusslandish and English | | |
| Remarks | The Maritime Search and Rescue Service is under the command of the Jusslander NAVY.  Attention is drawn to the International Code of Signals, Medical Section. | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **JUSSLAND MRCC** | | | | | | |
| 32°31′.50 S 60°54′.07 E | MMSI 005742029 | DSC VHF : Can 70  DSC MF : 2187,5 kHz  DSC HF4 : 4207,5 kHz  DSC HF6 : 6312,0 kHz  DSC HF8 : 8414,5 kHz  DSC HF12 : 12577,0 kHz  DSC HF16 : 16804,5 kHz | | AMVER |  | Diagram page 271 |
|  +999(0)1 23456789 | | |  +999(0)1 23456788 | | | |
|  | | | email: mrcc.jussland@jussland.gov.js | | | |
| Inmarsat C : +583 422123456  TELEX : +998 123456 | | | WEBSITE : www.jussland.mrcc.js | | | |
| NOTES : 1. This station does not accept public correspondence, accepting Distress, Urgency and Safety traffic only..  2. Station accepts JUSSREP messages. | | | | | | |
| **VHF** |  |  |  |  |  |  |
|  | Ch 16 | | | | H24 | |
| **RT (MF)** |  | | | |  | |
|  | Transmits | | Receives | | Hours of watch | |
|  | 2182 | | 2182 | | H24 | |
|  | 8291 | | 8291 | | H24 | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **BONBONKREMA MRSC** | | | | | | |
| 32°21′.70 S 60°55′.90 E | MMSI 005742030 | DSC VHF : Can 70  DSC MF : 2187,5 kHz  DSC HF4 : 4207,5 kHz  DSC HF6 : 6312,0 kHz  DSC HF8 : 8414,5 kHz  DSC HF12 : 12577,0 kHz  DSC HF16 : 16804,5 kHz | | AMVER |  | Diagram page 271 |
|  +999(0)1 23456790 | | |  +999(0)1 23456789 | | | |
|  | | | email: mrsc.jussland@jussland.gov.js | | | |
| NOTES : 1. This station does not accept public correspondence, accepting Distress, Urgency and Safety traffic only..  2. Station accepts JUSSREP messages. | | | | | | |
| **VHF** |  |  |  |  |  |  |
|  | Ch 16 74 | | | | H24 | |
| **RT (MF)** |  | | | |  | |
|  | Transmits | | Receives | | Hours of watch | |
| Kipassebien  32°26′.80 S 60°55′.70 E | 2182 | |  | |  | |
| 8291 | |
| Jentendlamer  32°33′.40 S 60°49′.50 E |  | | 2182 | | H24 | |
| 8291 | | H24 | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **BONBONKREMA (ZZZ) [9999]** | | | | | | |
| 32°23′.30 S 60°57′.20 E | MMSI 005742031 | DSC VHF : Can 70  DSC MF : 2187,5 kHz  DSC HF6 : 6312,0 kHz  DSC HF8 : 8414,5 kHz | | AMVER |  | Diagram page 271 |
|  +999(0)1 51365017 & 36502642 | | |  +999(0)1 51136501 | | | |
| CALL : Krema Radio | | | email: mickleradio@jussland.js | | | |
| Inmarsat C : +583 422123457  Iridium phone : +991 621461635  TELEX : +998 441200 BBKRM | | |  | | | |
| NOTES : 1. Accepts **Ship’s Weather Reports** adressed to CENMETEOKREM.  2. Station accepts AMVER messages.  3. Station accepts JUSSREP messages. | | | | | | |
| **VHF** |  |  |  |  |  |  |
| Chamalow | Ch 16 27 | | | | 32°37′.05 S 60°52′.40 E | |
| Caramelmou | Ch 16 | | | | 32°30′.40 S 60°57′.90 E | |
| Pastilledezan | Ch 14 16 24 33 | | | | 32°21′.10 S 60°55′.04 E | |
| NOTE : Pastlledezan in service only during the summer period (15th Oct. to 15th Mar). | | | | | | |
| **DSC** |  | | | |  | |
|  | Transmits | | Receives | | Hours of Watch | |
| **Public Correspondance** | 2189.5 | | 2177 | | 2300-1500 | |
|  | |  | |  | |
| **RT (MF)** |  | | | |  | |
|  | Transmits | | Receives | | Hours of Watch | |
|  | 2182 | | 2182 | | 2200-1000 | |
|  | 3180 | | 2080 | |  | |
| **RT (HF)** |  |  |  |  |  |  |
|  | Transmits | | Receives | | Hours of Watch | |
|  | 7903 | | 7903 | | H24 | |
| 7972 | | 7972 | |  | |
| 8125 | | 8125 | |
| 8131 | | 8131 | |
| 8140 | | 8140 | |
| 8176 | | 8176 | |
| 8294 | | 8294 | |
| 8755 *(Ch 813)* | | 8231 | |
| 11456 | | 11456 | |
| **12359** | | 12359 | | H24 | |
| 12365 | | 12365 | |  | |
| TRAFFIC LISTS: 12359 kHz: 0003 0203 0803 1003 1603 1803 | | | | | | |
| **Radiotelex [9999]** |  | |  | | | |
|  | Transmits | | Receives | | Hours of Watch | |
|  | 2174.5 | | 2174.5 | | 2300-1500 | |
|  | 6317 | | 6265 | | 0100-0500 | |
|  | 8376.5 | | 8376.5 | | 2300-1500 | |
| **WT (MF)** |  | |  | |  | |
|  | Transmits | | Receives | | Hours of Watch | |
|  | **458** 500 | | 500 | | 2300-1500 | |
| TRAFFIC LISTS: 458 kHz: 0000 0400 0800 1200 2300 | | | | | | |
| **WT (HF)** | | | | | | |
|  | Transmits | | Receives | | Hours of Watch | |
|  | 6337 | | 6 MHz (6 9) ???? | | 0500-0600 | |
|  | 8461 | | 8 MHz (8 9) ???? | | 0000-0100 0400-0500 | |
|  | 12970.5 | | 12 MHz (3 9) ???? | | 0100-0200 | |
| TRAFFIC LISTS: 8461 kHz: 000 0400 | | | | | | |
| **Data Service (HF)** | | | | | | |
| Channel ??? | Dial Frequency Rx | | Dial Frequency Tx | | Hours | |
| KREM10 | 8716 | | 8716 | | H24 | |
| KREM11 | 13078.5 | | 13078.5 | | On request | |
| KREM12 | 17198.5 | | 17198.5 | |
| KREM13 | 22567.5 | | 22567.5 | | H24 | |
| Bonbonkrema provides data services in partnership with Swisscom Maritimes Communications. | | | | | | |

MARITIME SAFETY INFORMATION SERVICES

RADIO WEATHER SERVICES AND NAVIGATIONAL WARNINGS

|  |
| --- |
| **METEOROLOGICAL AND HYDROLOGICAL INFORMATION TRANSMITTED THROUGH THE AUTOMATIC IDENTIFICATION SYSTEM (AIS)** |

The Jussland Transport Agency transmits AIS messages containing meteorological and hydrological information in all sea areas within VHF range of the Jussland AIS base network

The message contains weather data from the wind and water level gauges closest to the vessel receiving the messages. Receipt of the message on AIS is possible only if the AIS device contains a program with the required specification.

|  |  |  |
| --- | --- | --- |
| **INTERNET WEATHER SERVICES** | | |
| www.meteojussland.js | Jussland Met Office | Marine weather forecast for Jussland waters |

|  |  |  |  |
| --- | --- | --- | --- |
| **NAVTEX** | | | |
| **J** | Caramelmou | 518 kHz | 32°30′.40 S 60°57′.90 E |
| **N** | Chamalow | 32°37′.05 S 60°52′.40 E |
| **D** | Pastilledezan | 490 kHz | 32°21′.10 S 60°55′.04 E |
| **Weather Bulletins** | | | |
| **J** : 0830 2030 | Storm warning, synoptic situation and development and forecast valid for 24 hours within 450 n miles of coast. | | |
| **J** : 0900 2100 | Storm warning, weather bulletin. | | |
| **N** : 1000 2200 | Storm warning, synoptic situation and development and forecast valid for 24 hours within 450 n miles of coast. | | |
| **N** : 1030 2230 | High sea forecast. Ice forecast. | | |
| **D** : 1200 2400 | Weather bulletin for coastal water. | | |
| **Navigational Warning** | | | |
| **J** : 0030 0830 1230 2030 | NAVAREA VII and coastal warning. | | |
| **J** : 0100 0900 1300 2100 | Navigational Warning. | | |
| **N** : 0200 1000 1400 2200 | NAVAREA VII and coastal warning. | | |
| **N** : 0230 1030 1430 2230 | Navigational Warning. Ice forecast. | | |
| **D** : 0400 1200 1600 2400 | NAVAREA VII and coastal warning. | | |
| **D** : 0430 1230 1630 2400 | Navigational Warning. | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **BONBONKREMA MRSC** | | |  | | **32°21′.70 S 60°55′.90 E** | |
|  | Ch 74 | VHF | |  | |  |
| **Weather Bulletins** | | | | | | |
| 0033 0433 0833 1233 2033 | Coastal waters forecast in English. Gale warnings for coastal waters. | | | | | |
| 0233 0633 1033 1433 1833 2233 | High seas forecast in English. Gale warnings for high seas. | | | | | |
| On receipt | Storm warnings. | | | | | |
| **Navigational Warning** | | | | | | |
| 0033 0433 0833 1233 2033 | Navigational warnings after weather bulletins. | | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **BONBONKREMA (ZZZ) [9999]** | | | **32°23′.30 S 60°57′.20 E** | | |
| **A** | 3180 | RT (MF) | | Bonbonkrema | 32°23′.30 S 60°57′.20 E |
| **B** | Ch 27 | VHF | | Chamalow | 32°37′.05 S 60°52′.40 E |
| Ch 23 | Caramelmou | 32°30′.40 S 60°57′.90 E |
| Ch 14 | Pastilledezan | 32°21′.10 S 60°55′.04 E |
| **Weather Bulletins** | | | | | |
| **A** : 0750 1950 | Weather synopsis and 24 hour forecast, storm warnings. | | | | |
| **A** : 1303 | Weather synopsis and 48 hour forecast, storm warnings. | | | | |
| **B** : 0910 2110 | Weather warnings and 48 hours forecast for coastal waters. | | | | |
| **Navigational Warning** | | | | | |
| **A** : 0750 1950  **B** : 0910 2110 | Navigational warnings after weather bulletins. | | | | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **JUSSLAND RADIO** | | |  | | |
| **A** | 193 | LW | | Jussland City |  |
| **B** | 1485 | MW | | Chamalow |  |
| 720 | Caramelmou |  |
| 774 | Pastilledezan |  |
| **C** | 104.9 MHz | FM | |  |  |
| **Weather Bulletins** | | | | | |
| **A-C** : 0048 0520 LT | Gale warnings, High sea forecast, weather reports from coast stations and the coastal forecast. | | | | |
| **A** : 1201 1754 LT | Gale warnings and High sea forecast. | | | | |
| **C** : 1754 LT (Sat & Sun) |

**RADIO-FACSIMILE**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **BONBONKREMA** | | | | | | **32°23′.30 S 60°57′.20 E** | | | |
|  | | 6446 | | | |  | | | H24 |
|  | | 7907 | | | |  | | | 1900-0600 |
|  | | 8444 | | | |  | | | HN |
| **Map Areas** | | | | | | | | | |
| A | 1:5,000,000  32°S.60°E 32°S.65°E  34°S.60°E 34°S.65°E | | | B | 1:5,000,000  24°S.60°E 24°S.70°E  32°S.60°E 32°S.70°E |  |  | | |
| **Schedule** | | | | | | | | | |
| A | | | 36 hour surface prognosis | | | 0700 (00) | | 120/576 | |
| A | | | Sea state analysis | | | 0800 (06) | |
| B | | | 36 hour surface prognosis | | | 1000 (06) | |
| A | | | Surface temperature analysis / iceberg positions | | | 1400 (12) | |
| B | | | Sea state analysis | | | 1500 (12) | |
| ?? | | | Broadcast schedule | | | 1850 | | 90/576 | |
| ?? | | | Iceberg prognosis | | | 2000 | | 120/576 | |

**SAFETYNET**

**EGC SAFETYNET SYSTEM**

Transmission schedule for full GMDSS service

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **NAVAREA** | **NAV information** | | **METAREA** | **MET information** | |
| **Coordinator** | **Times (UTC)** | **Issuing country** | **Times (UTC)** |
| **I** | United Kingdom | 0530, 1730 (AOR-E) | **I** | United Kingdom | 0930, 2130 (AOR-E)  Warnings only on receipt (AOR-W) |
| **II** | France | 0430, 1630 (AOR-E) | **II** | France | 1015, 2215 (AOR-E / AOR-W) |
| **III** | Spain | 1200, 2400 & on receipt (AOR-E) | **III** | Greece1 | 1000, 2200 (AOR-E) |
| **IV** | United States | 1000, 2200 (AOR-W)  (1200 Ice reports N Atlantic)  0900, 2100 (AOR-W) French West Indies  0900, 2100 (AOR-W) French Guyana | **IV** | United States | 0430, 1030, 1630, 2230 (AOR-W) |
| **V** | Brazil | 0030, 1230 (AOR-E) | **V** | Brazil | 0730, 1930 (AOR-E) |
| Coastal warnings for Amazon Basin and additional coastal areas (AOR-E) |
| **VI** | Argentina | 0200, 1400 (AOR-W) | **VI** | Argentina | 0230, 1730 (AOR-W) |
| **VII** | South Africa | 1940 (AOR-E / IOR)  0140, 1340 (IOR) Kerguelen Islands  0330, 1530 (IOR) Mayotte  0400, 1600 (IOR) Jussland | **VII** | South Africa | 0940, 1940, (AOR-E / IOR)2, 5 |
| **VIII** | India | 1000, 2200 (IOR)  0040, 1240 (IOR) Réunion  0330, 1530 (IOR) Mayotte | **VIII (N)** | India | 0900, 1800 for N of 0° (IOR) |
| **VIII (S)** | Mauritius / Réunion | 0130, 1330 for S of 0° (IOR)  00003, 06003, 12003, 18003 for S of 0° (IOR) |
| Australia | warnings only for S of 0° and E of 90°E (IOR) |
| **IX** | Pakistan | 0800 (IOR) | **IX** | Pakistan | 0700 (IOR) |
| **X** | Australia | 0700, 1900 & on receipt (IOR / POR)  0140, 1340 (POR) New Caledonia | **X** | Australia | 1030, 2330 (IOR) |
| 1100, 2300 (POR) |
| Coastal Warnings for Bass Strait, Northern Territory & Western Australia (IOR / POR) |
| **XI** | Japan | 0005, 1205 (POR / IOR) | **XI** | China | 0330, 1015, 1530, 2215 (IOR) |
| Japan | 0230, 0830, 1430, 2030 for N of 0° (POR)  0815, 20154 for S of 0° (POR) |
| **XII** | United States | 1030, 2230 (POR / AOR-W) | **XII** | United States | 0545, 1145, 1745, 2345 (POR / AOR-W) |
| **XIII** | Russian Federation | 0930, 2130 (POR) | **XIII** | Russian Federation | 0930, 2130 (POR) |
| **XIV** | New Zealand | 0900, 2100 (POR) New Zealand  0140, 1340 (POR) New Caledonia  0030, 1230 (POR) Wallis & Futuna  0250, 1450 (POR) French Polynesia | **XIV** | New Zealand | 0330, 0930, 1530, 2130 (POR) Warnings  0330, 1530, (POR) for Area Southern  0930, 2130 (POR) for Area Subtropic, Forties & Pacific |
| **XV** | Chile | 0210, 1410 (AOR-W) | **XV** | Chile | 0100, 1330 (AOR-W) for Sea Areas 1-8  1440 (AOR-W) for Sea Area 9  0345, 1845 (AOR-W) for Sea Area 10 |
| **XVI** | Peru | 0500, 1700 (AOR-W) | **XVI** | United States | 0515, 1115, 1715, 2315 (AOR-W) |
| **XVII** | Canada | 1130, 2330 (POR) | **XVII** | Canada | 0300, 1500 (POR) |
| **XVIII** | Canada | 1100, 2300 (AOR-W) | **XVIII** | Canada | 0300, 1500 (AOR-W) |
| **XIX** | Norway | 0630, 1830 (AOR-E) | **XIX** | Norway | 1100, 2300 (AOR-E) |
| **XX** | Russian Federation | 0530, 1730 (IOR) | **XX** | Russian Federation | 0600, 1800 (IOR) |
| **XXI** | Russian Federation | 0630, 1830 (POR) | **XXI** | Russian Federation | 0600, 1800 (POR) |

**1** Scheduled bulletins and warnings for Western Mediterranean Sea are prepared by France.

**2** Forecasts for areas 30°S - 50°E / 50°S - 80°E and tropical cyclone warnings are prepared by Réunion.

**3** Tropical cyclone warnings (if any) issued by Réunion as an unscheduled broadcast.

**4** Scheduled bulletins and warnings for south of the equator prepared by Australia.

5 Transmission via AOR-E for areas West of 20°E, transmission via IOR for areas East of 20°E.

GLOBAL MARITIME DISTRESS AND SAFETY SYSTEM (GMDSS)

**SEA AREA A1**

|  |
| --- |
| **VHF DSC, LIST OF COAST STATIONS FOR SEA AREA A1** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Country**  Station | MMSI | Position | Range  (n miles) | Status*(Associated RCCs)* |
| (1) | (2) | (3) | (4) | (5) |
| **Jussland** |  |  |  |  |
| Jussland | 005742029 | 32°31′.50 S 60°54′.07 E | 50 | Operational *(MRCC Jussland)* |
| Bonbonkrema MRSC | 005742030 | 32°21′.70 S 60°55′.90 E | 50 | Operational *(MRCC Jussland)* |
| Bonbonkrema (ZZZ)  Remotely controlled stations :  Chamalow  Caramelmou  Pastilledezan | 005742031 | 32°23′.30 S 60°57′.20 E  32°37′.05 S 60°52′.40 E  32°30′.40 S 60°57′.90 E  32°21′.10 S 60°55′.04 E | 50  50  50  50 | Operational *(MRCC Jussland)* |

**SEA AREA A2**

|  |
| --- |
| **MF DSC, LIST OF COAST STATIONS FOR SEA AREA A2** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Country**  Station | MMSI | Position | Range  (n miles) | Status*(Associated RCCs)* |
| (1) | (2) | (3) | (4) | (5) |
| **Jussland** |  |  |  |  |
| Jussland | 005742029 | 32°31′.50 S 60°54′.07 E | 150 | Operational *(MRCC Jussland)* |
| Bonbonkrema MRSC | 005742030 | 32°21′.70 S 60°55′.90 E | 150 | Operational *(MRCC Jussland)* |
| Bonbonkrema (ZZZ) | 005742031 | 32°23′.30 S 60°57′.20 E | 150 | Operational *(MRCC Jussland)* |

**SEA AREAS A3/A4**

|  |
| --- |
| **HF DSC, LIST OF COAST STATIONS FOR SEA AREAS A3 AND A4** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Country**  Station | MMSI | Operational frequency bands | Range  (n miles) | Status*(Associated RCCs)* |
| (1) | (2) | (3) | (4) | (5) |
| **Jussland** |  |  |  |  |
| Jussland | 005742029 | 4,6,8,12 & 16 MHz | 150 | Operational *(MRCC Jussland)* |
| Bonbonkrema MRSC | 005742030 | 4,6,8,12 & 16 MHz | 150 | Operational *(MRCC Jussland)* |
| Bonbonkrema (ZZZ) | 005742031 | 4,6,8,12 & 16 MHz | 150 | Operational *(MRCC Jussland)* |

**MSI**

|  |
| --- |
| **MARITIME SAFETY INFORMATION (MSI) UNDER THE GMDSS** |

HF NBDP MARITIME SAFETY INFORMATION BROADCAST SERVICE

|  |  |  |  |
| --- | --- | --- | --- |
| **BONBONKREMA (ZZZ) [9999]** | | | **32°23′.30 S 60°57′.20 E** |
| **A** | 8416.5 | RADIO-TELEX | |
| **B** | 16806.5 |
| **Weather Bulletins** | | | |
| **A** : 0000 1130 | Meteorogical warnings. | | |
| **B** : 0030 1200 |
| **Navigational Warning** | | | |
| **A** : 0000 1130 | Navigational warnings. | | |
| **B** : 0030 1200 |

**NAVAREA COORDINATORS**

**NAVAREA VII (South Africa)**

The Hydrographer, S.A. Navy

Hydrographic Office

private Bag X1, Tokai

7966 CAPE TOWN

South Africa

Telephone : +27 21 7872408

Fax : +27 21 7872228

email : hydrosan@iafrica.com

Website : http//www.sanho.co.za

**National Coordinators**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **COUNTRY** | **TELEPHONE** | **FACSIMILE** | **EMAIL** | **OTHER** |
| **Angola** | +244 22 2449211 | +244 22 2447320 | hidroportos@netangola.com |  |
| **Jussland** | +999(0)1 23451111 | +999(0)1 23451112 | hidrojussland@jussland.gov.js |  |
| **Madagascar** |  |  |  |  |
| **Mozambique** | +258 1 430186 | +258 1 430185 | hidro@inahina.uem.mz |  |
| **Namibia** | +264 64 2082258 | +264 64 2082326 | mmandia@namport.com.na |  |

**SAR**

**JUSSLAND**

|  |  |  |  |
| --- | --- | --- | --- |
| **National SAR Agency** : HQ Jusslander NAVY  **Adresse**: Spring Place, 105 Commercial Road, Jussland City  JS5629 JUSSLAND  **Tel**: +999 (0)1 56489652 (Office hours only)  **Fax**: +999 (0)1 56894123 (Office hours only)  **email**: sar.response@jussland.gov.js | | | |
| **TeleMedical Assistance Service** : The Jussland city Hospital provides assistance. Contact via any radiostations requesting Medico assistance. | | | |
|  | **Telephone** +999 | **Fax** + 999 | **Other** |
| Jussland MRCC | (0)1 23456789 | (0)1 23456788 | Inmarsat-C : +583 422123456  TELEX : +998 123456  email : mrcc.jussland@jussland.gov.js |
| Bonbonkrema MRSC | (0)1 23456790 | (0)1 23456789 | email : mrsc.jussland@jussland.gov.js |
| Bonbonkrema (ZZZ) | (0)1 51365017  (0)1 36502642 | (0)1 51136501 | email : mickleradio@jussland.js |